|  |
| --- |
| **Heat pump water heater** |
|
| Model: | HEATANK V2 200 |
| Manufacturer: | EUROFRED S.A. |
| Address: | Cl. Marqués de Sentmenat, 97 - 08029 Barcelona - Spain |
| Denomination : | HOT WATER HEAT PUMP |
| Intended use: | hot water |
| Power supply: | Ph/V/Hz | 230V~ 50Hz |
| Assembly type: | single package |
| Refrigerant : | R134a/ 1200g |
| The water heating energy efficiency ηwh : | (%) | 126.6 |
| The energy efficiency class of the model, determined in accordance with point 1 of Annex II |  | Class A |
| The annual electricity consumption AEC: | kWh/annum | 809 |
| The daily electricity consumption Qelec: | kWh | 3.854 |
| The sound power level in dB (indoors）: | dB | 59 |
| Mixed water at 40 °C V40  | L | 243 |
| Load profiles of water heaters, Type: |  | L |

**Load profiles of water heaters :**

|  |  |
| --- | --- |
| 　h | L |
| *Qtap* | *f* | *Tm* | *Tp* |
| kWh | l/min | ℃ | ℃ |
| 7:00 | **0.105** | 3 | 25 | 　 |
| 7:05 | **1.4** | 6 | 40 | 　 |
| 7:30 | **0.105** | 3 | 25 | 　 |
| 7:45 | **0.105** | 3 | 25 | 　 |
| 8:05 | **3.605** | 10 | 10 | 40 |
| 8:25 | **0.105** | 3 | 25 | 　 |
| 8:30 | **0.105** | 3 | 25 | 　 |
| 8:45 | **0.105** | 3 | 25 | 　 |
| 9:00 | **0.105** | 3 | 25 | 　 |
| 9:30 | **0.105** | 3 | 25 | 　 |
| 10:30 | **0.105** | 3 | 10 | 40 |
| 11:30 | **0.105** | 3 | 25 | 　 |
| 11:45 | **0.105** | 3 | 25 | 　 |
| 12:45 | **0.315** | 4 | 10 | 55 |
| 14:30 | **0.105** | 3 | 25 | 　 |
| 15:30 | **0.105** | 3 | 25 | 　 |
| 16:30 | **0.105** | 3 | 25 | 　 |
| 18:00 | **0.105** | 3 | 25 | 　 |
| 18:15 | **0.105** | 3 | 40 | 　 |
| 18:30 | **0.105** | 3 | 40 | 　 |
| 19:00 | **0.105** | 3 | 25 | 　 |
| 20:30 | **0.735** | 4 | 10 | 55 |
| 21:00 | **3.605** | 10 | 10 | 40 |
| 21:30 | **0.105** | 3 | 25 | 　 |
| *Qref* | 11.655 |